**Emerging Rare earth perovskite nanostructures for energy conversion**

**B. Dirrouch1, H. Jebari2 , M.Y. Messous3, H. Zalrhi1 , M. Regragui1, H. Ez-Zahraouy2, M. Abdlefdil1, L. Atourki1**

1 MANAPSE Lab, Faculty of Science, Mohammed V University in Rabat, Morocco.

2 Laboratory of Condensed Matter and Interdisciplinary Sciences, Unite de Recherche Labialisées CNRST, URL-CNRST17, Faculty of Sciences, Mohammed V University in Rabat, Morocco.

3 Materials Science unit (USM/DERS), National Center for Energy, Sciences and Nuclear Techniques -CNESTEN-, Rabat, Morocco.

Email: badr.dirrouch@um5r.ac.ma / l.atourki@um5r.ac.ma

**Abstract**: This study focuses on synthesizing nanoparticles of the rare-earth perovskite LaFeO3 (LFO) with varying Ytter bium (Yb) doping levels using the co-precipitation method. All samples crystallized in the orthorhombic perovskite phase, with crystallite sizes ranging between 36.3 and 37.5 nm. The nanoparticles exhibited a rela tively uniform distribution across the sample surface, and their chemical composition aligned precisely with the stoichiometric composition of LaFeO3, as confirmed quantitatively. A comparative investigation of the structural and electronic properties of La1-*x*Yb*x*FeO3 nanoparticles (*x* =0.00 to 0.04) is also performed in this manuscript. Optical bandgap energies, determined via computational investigation, were 2.30 eV and 2.06 eV following [100] and [001] directions, respectively. Afterward, this parameter was reduced to 2.14 eV and 2.06 eV (along [100] and [001] directions, respectively) by adding 4 % of Yb at La sites. LFO compound exhibits indirect bandgap energies with p-type semiconductor behavior. The unique properties of the synthesized LFO nano particles suggest their potential application in photoelectrochemical water splitting, catalysis, gas sensing, and energy conversion devices

**Keywords**: Rare-earth perovskites; LaFeO3 nanoparticles; Co-precipitation technique; Computational Investigation; Energy conversion devices.